{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Planilha1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Planilha1","index":0,"n_rows":11,"n_cols":15,"rows_kept":11,"cut":false,"hidden":false,"merged":[[10,4,10,7],[10,10,10,13],[8,1,8,2],[9,1,9,2],[6,1,6,2],[7,1,7,2],[4,1,4,2],[5,1,5,2],[1,9,1,14],[2,10,2,11],[2,12,2,13],[2,14,3,14],[0,0,0,14],[2,0,3,2],[2,4,2,5],[2,6,2,7],[2,8,3,8],[1,3,1,8],[1,0,1,2]]}
["4.2.3. 4011209 - Regularização do subleito (m²)"]
[null,null,null,"CODEVASF",{"$nulls":5},"TR ENGENHARIA"]
["EQUIPAMENTOS",null,null,"QUANT","UTILIZAÇÃO",null,"CUSTO OPERACIONAL",null,"CUSTO HORÁRIO","QUANT","UTILIZAÇÃO",null,"CUSTO OPERACIONAL",null,"CUSTO HORÁRIO"]
[{"$nulls":4},"PROD","IMPR","PROD","IMPR",null,null,"PROD","IMPR","PROD","IMPR"]
["E9571","Caminhão tanque com capacidade de 10.000 l - 188 kW",null,2,0.51,0.49,128.0966,31.772400000000001,254.66821600000003,1,0.76,0.24,128.0966,31.772400000000001,104.97880000000001]
["E9518","Grade de 24 discos rebocável de 24\"",null,1,0.69,0.31,1.4624999999999999,0.9627,1.3075619999999999,1,0.52,0.48,1.4624999999999999,0.9627,1.2225999999999999]
["E9524","Motoniveladora - 93 kW",null,1,0.71,0.28999999999999998,110.89490000000001,46.4846,92.215913,1,0.55000000000000004,0.45,110.89490000000001,46.4846,81.910300000000007]
["E9762","Rolo compactador de pneus autopropelido de 27 t - 85 kW",null,1,0.96,0.04,86.636399999999995,40.851500000000001,84.805003999999997,1,0.72,0.28000000000000003,86.636399999999995,40.851500000000001,73.816599999999994]
["E9685","Rolo compactador pé de carneiro vibratório autopropelido de 11,6 t - 82 kW",null,1,1,0,84.644099999999995,37.498199999999997,84.644099999999995,1,1,0,84.644099999999995,37.498199999999997,84.644099999999995]
["E9577","Trator agrícola - 77 kW",null,1,0.69,0.31,81.123599999999996,21.444900000000001,62.623202999999997,1,0.52,0.48,81.123599999999996,21.444900000000001,52.477899999999998]
[{"$nulls":4},"TOTAL EQUIPAMENTOS:",null,null,null,{"$f":"SUM(I5:I10)","v":580.26399800000002},null,"TOTAL EQUIPAMENTOS:",null,null,null,{"$f":"SUM(O5:O10)","v":399.05029999999999}]